Hydro-X Xtreme Xtractor **Troubleshooting**

**Unit will not operate:**

1. Unit is plugged in.
2. No Power - Check outlet and home circuit breakers with circuit tester – change outlets.
3. Blown Fuse or Open Breaker - reset circuit breaker or replace blown fuse.
4. GFCI Tripped - After plugging in GFCI and machine power cord, press “RESET” button on GFCI
5. Turn unit power switch from on to off and back to on.
6. Inspect unit power cords, unplug and re-plug all connections.
7. Loose power connections on machine at Motor Connections – reseat handle to motor lead connection.