**Troubleshooting DriEaz Hepa 500 Air Scrubber**

**Unit does not operate**

1. No Power to machine – check that the unit is plugged in – use another outlet if needed
2. Switch not turned on – turn on power switch
3. No power to outlet – reset circuit breaker/GFCI

**Change light illuminated**

1. Primary filter is full – replace filters
2. Air intake restricted – eliminate bends/kinks in ducting or remove ducting

**Blower wheel not turning**

1. Obstructed blower – remove obstruction
2. Loose blower wheel set screw – tighten set screw
3. Blower damaged or defective – inspect and repair or replace blower as needed