**Troubleshooting Phoenix Air Movers**

**Power switch is on but No air flow, fan is not turning and switch does not light when ON.**

1. Unit is unplugged or no power to outlet – plug in to outlet or use a different outlet
2. Unit circuit breaker or GFI breaker has been triggered – reset or replace breaker
3. Power cord or extension cord is damaged or defective – replace cord(s)

4. Power switch defective – replace switch

5. Loose connection in internal wiring – repair wiring

**Power switch and light are on but No air flow, fan is not turning.**

1. Power switch is defective – replace power switch

2. Internal wiring has loose connection or wiring is damaged – repair wiring

3. Fan motor is defective – repair or replace motor