**Troubleshooting Phoenix Firebird TX80**

**Blower not running**

1. Unit unplugged or no power to outlet – plug in to outlet or use a different outlet
2. Power Switch not working – repair or replace
3. Thermostat not calling for heat – test thermostat and replace as needed.
4. Wiring fault inside device – inspect and repair wiring
5. Defective blower or blower capacitor – test and replace as needed

**Blower running but no heat**

1. Airflow restricted at inlet or outlet or fouled coil – removed restrictions and or clean or replace coil.
2. Heating source not operating – test and repair or replace wiring or components as needed.