**Basic Troubleshooting Air Movers**

**Power switch is on but No air flow, fan is not turning and switch does not light.**

1. Unit is unplugged – plug in unit cord to wall outlet
2. No power to outlet – use a different outlet if available
3. Wall outlet circuit breaker or GFI breaker has been tripped – reset breaker
4. Power cord or extension cord is damaged or defective – replace cord(s)

4. Power switch damaged or defective – take to service center to replace switch

5. Loose connection or damage to internal wiring – take to service center for wiring repair

**Power switch and light are on but No air flow, fan is not turning.**

1. Power switch is defective – take to service center to replace power switch

2. Internal wiring has loose connection or wiring is damaged – take to service center to repair wiring

3. Fan motor is damaged or defective – take to service center to repair or replace motor